**Soffit element extension Duo LEV**

Extension for Duo LE soffit element for installation in the window soffit.

Is required as an optional accessory when installing in the window soffit.

Technical data

|  |  |
| --- | --- |
| Article: | Duo LEV |
| Air flow volume: | 60 m³/h |
| Material: | Aluminium/stainless steel |
| Colour: | Aluminium, not painted |
| Weight: | 2,42 kg |
| Weight including packaging: | 3,11 kg |
| Width: | 1.000 mm |
| Height: | 410 mm |
| Depth: | 64 mm |
| Width with packaging: | 1.010 mm |
| Height with packaging: | 455 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799930891 |
| Article number: | 0093.0089 |

Manufacturer: MAICO

Duo LEV Soffit element extension