**Quickbox ESQ 40/4 K**

Model

230 V model.

Speed controllable with transformer.

Prescribed motor overload switch must be provided by customer.

Features

Side panel with exhaust air connection can be fitted in 3 different directions. Can therefore be varied during installation even in awkward spaces.

Compact dimensions.

Motor located outside of the air flow.

Very quiet operation thanks to excellent sound insulation.

Impeller with blades curved to the rear. Resulting in optimised efficiency and low maintenance costs.

IP 55 degree of protection.

Mounting instructions

Installation inside the building.

Mounting feet already pre-fitted.

Side section with intake socket is permanently fitted. The side section with exhaust opening can be adapted to a wide range of installation situations.

Housing wall is easy to remove.

S Information sign - Impeller direction of rotation

T Rating plate

Electrical connection

Connection to external terminal box.

Technical data

|  |  |
| --- | --- |
| Article: | ESQ 40/4 K |
| Air flow volume: | 4.500 m³/h |
| Speed controllable: | ✔ |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 550 W |
| PMax: | 550 W |
| Inom: | 4,75 A |
| Imax: | 4,8 A |
| Degree of protection: | IP 55 |
| Insulation class: | F |
| Mains cable: | 3 x 1,5 mm² |
| Housing material: | Sheet steel, galvanised |
| Weight: | 64 kg |
| Weight including packaging: | 64,49 kg |
| Swivelling fan: | - |
| Nominal size: | 400 mm |
| Width with packaging: | 742 mm |
| Height with packaging: | 792 mm |
| Depth with packaging: | 652 mm |
| Airstream temperature at nominal current: | 180 °C |
| Airstream temperature at IMax: | -10 °C up to 180 °C |
| Sound pressure level: | 49 dB(A) Distance 3 m, Free-field conditions |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799800729 |
| Article number: | 0080.0072 |

Manufacturer: MAICO

ESQ 40/4 K Quickbox