**Room air control RLS G1 WS**

Design room air control included in the scope of delivery of the WS 75 Powerbox S and H ventilation units.

Optional as an accessory for WS 120 Trio, WS 160 Flat, WS 170, WS 300 Flat, WR 310 / WR 410, WS 320 and WS 470 ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | RLS G1 WS |
| Type of voltage: | Alternating current |
| Rated voltage: | 12 V |
| Material: | Glass |
| Colour: | White |
| Weight: | 0,16 kg |
| Weight including packaging: | 0,25 kg |
| Width: | 130 mm |
| Height: | 92 mm |
| Depth: | 15 mm |
| Width with packaging: | 265 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 49 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992516 |
| Article number: | 0157.1593 |

Manufacturer: MAICO

RLS G1 WS Room air control