**Air filter, replacement PPF E2**

Replacement air filter for PushPull 60 K single-room ventilation unit

Technical data

|  |  |
| --- | --- |
| Article: | PPF E2 |
| Installation site: | Ventilation unit |
| Material: | Synthetic |
| Colour: | Black |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,07 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Width: | 190 mm |
| Height: | 170 mm |
| Depth: | 18 mm |
| Width with packaging: | 190,5 mm |
| Height with packaging: | 170,5 mm |
| Depth with packaging: | 40 mm |
| Packing unit: | 2 pieces |
| Range: | K |
| GTIN (EAN): | 4012799930860 |
| Article number: | 0093.0086 |

Manufacturer: MAICO

PPF E2 Air filter, replacement