**Channel sensor FL 30 P**

Temperature sensor for measuring the air temperature in air channels.

Can be combined with ETL 16 P, DTL 16 P, DTL 24 P.

Technical data

|  |  |
| --- | --- |
| Article: | FL 30 P |
| Degree of protection: | IP 20 |
| Installation site: | Channel |
| Material: | Synthetic material |
| Weight: | 0,08 kg |
| Weight including packaging: | 0,08 kg |
| Width: | 220 mm |
| Height: | 140 mm |
| Depth: | 20 mm |
| Width with packaging: | 221 mm |
| Height with packaging: | 141 mm |
| Depth with packaging: | 21 mm |
| Temperature setting range: | 0 °C up to 30 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799577805 |
| Article number: | 0157.0780 |

Manufacturer: MAICO

FL 30 P Channel sensor