**45° branch, horizontal AZ45H55/220/55/110**

Features

45° branch, horizontal, all exits collar size. Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | AZ45H55/220/55/110 |
| Material: | Sheet steel, Sendzimir galvanised |
| Channel dimension: | 220 mm x Array x 55 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799557579 |
| Article number: | 0055.0757 |

Manufacturer: MAICO

AZ45H55/220/55/110 45° branch, horizontal