**90° angle elbow, extended, left-sided asymmetrical WB90VLS/55/220/125**

Features

Square/round angle elbow, left-hand asymmetrical (all exits collar size). Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | WB90VLS/55/220/125 |
| Material: | Sheet steel, Sendzimir galvanised |
| Weight including packaging: | 0 kg |
| Nominal size: | 125 mm |
| Channel dimension: | 220 mm x Array x 55 mm |
| Width with packaging: | 0 mm |
| Height with packaging: | 0 mm |
| Depth with packaging: | 0 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799557531 |
| Article number: | 0055.0753 |

Manufacturer: MAICO

WB90VLS/55/220/125 90° angle elbow, extended, left-sided asymmetrical