**Power board DTL 2 P-L alt**

Additional board for installation in the DTL 24 P electronic temperature control to meet a power requirement of 16.5 kW to 30 kW.

Technical data

|  |  |
| --- | --- |
| Article: | DTL 2 P-L alt |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Weight: | 1,66 |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799577720 |
| Article number: | 0157.0772 |

Manufacturer: MAICO

DTL 2 P-L alt Power board