**Accessories for composite window ZD 31**

Mounting frame for installation of window fans in composite windows.

Opening and cleaning of double-glazed windows possible.

Outer pane spacing 20 mm to 40 mm.

Technical data

|  |  |
| --- | --- |
| Article: | ZD 31 |
| Installation site: | Window |
| Material: | Metal |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,7 kg |
| Suitable for nominal size: | 315 mm |
| Width: | 378 mm |
| Height: | 378 mm |
| Depth: | 8 mm |
| Width with packaging: | 390 mm |
| Height with packaging: | 390 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799939160 |
| Article number: | 0093.0916 |

Manufacturer: MAICO

ZD 31 Accessories for composite window