**Mounting foot FU 35**

Mounting feet for the assembly of EZL/DZL and EZR/DZR fans on walls, ceilings or brackets.

Technical data

|  |  |
| --- | --- |
| Article: | FU 35 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,56 kg |
| Weight including packaging: | 1,1 kg |
| Suitable for nominal size: | 350 mm |
| Width: | 319 mm |
| Height: | 100 mm |
| Depth: | 40 mm |
| Width with packaging: | 319 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 40 mm |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799360728 |
| Article number: | 0036.0072 |

Manufacturer: MAICO

FU 35 Mounting foot