**45° elbow, drawn B45-180**

45° elbow, drawn, incl. lip seal(s). For folded spiral-seam ducts.

Technical data

|  |  |
| --- | --- |
| Article: | B45-180 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Nominal size: | 180 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553298 |
| Article number: | 0055.0329 |

Manufacturer: MAICO

B45-180 45° elbow, drawn