**Accessories for composite window ZD 20-2**

Mounting frame for installation of window fans in composite windows.

Opening and cleaning of double-glazed windows possible.

Outer pane spacing 20 mm to 40 mm.

Technical data

|  |  |
| --- | --- |
| Article: | ZD 20-2 |
| Installation site: | Glass brick |
| Weight: | 0,085 |
| Weight including packaging: | 0,155 kg |
| Suitable for nominal size: | 200 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 65 mm |
| Depth with packaging: | 95 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799939139 |
| Article number: | 0093.0913 |

Manufacturer: MAICO

ZD 20-2 Accessories for composite window