**90° channel connector with O-ring gasket KS 160**

Technical data

|  |  |
| --- | --- |
| Article: | KS 160 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799554592 |
| Article number: | 0055.0459 |

Manufacturer: MAICO

KS 160 90° channel connector with O-ring gasket