**Air filter, replacement FF 133**

FF 133: Replacement air filter for UPR 133 exhaust fan.

Technical data

|  |  |
| --- | --- |
| Article: | FF 133 |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,06 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Width: | 125 mm |
| Height: | 125 mm |
| Depth: | 16 mm |
| Width with packaging: | 120 mm |
| Height with packaging: | 120 mm |
| Depth with packaging: | 75 mm |
| Packing unit: | 5 pieces |
| Suitable for products: | UPR 133 |
| Range: | B |
| GTIN (EAN): | 4012799930198 |
| Article number: | 0093.0019 |

Manufacturer: MAICO

FF 133 Air filter, replacement