**Axial duct fan DZR 40/6 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZR 40/6 A-Ex |
| Air flow volume: | 2.800 m³/h |
| Rotating speed: | 975 1/min |
| Nominal output: | 150 W |
| Inom: | 0,63 A |
| Imax: | 0,67 A |
| Weight: | 16,2 |
| IA/IN: | 2,5 |
| Certified as explosion proof: | 84/3894 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799867753 |
| Article number: | 0086.0775 |

Manufacturer: MAICO

DZR 40/6 A-Ex Axial duct fan