**90° elbow, drawn B90-180**

90° elbow, drawn, incl. lip seals. For folded spiral-seam ducts.

Technical data

|  |  |
| --- | --- |
| Article: | B90-180 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Nominal size: | 180 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553151 |
| Article number: | 0055.0315 |

Manufacturer: MAICO

B90-180 90° elbow, drawn