**90° channel elbows, long, vertical KB90LV/80/100**

Features

Long channel elbow, vertical, collar size. Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | KB90LV/80/100 |
| Material: | Sheet steel, Sendzimir galvanised |
| Weight including packaging: | 0 kg |
| Channel dimension: | 100 mm x Array x 80 mm |
| Width with packaging: | 0 mm |
| Height with packaging: | 0 mm |
| Depth with packaging: | 0 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799555797 |
| Article number: | 0055.0579 |

Manufacturer: MAICO

KB90LV/80/100 90° channel elbows, long, vertical