**45° channel elbows, horizontal KB45H/55/110**

Features

Horizontal channel elbow, collar size. Surface: Sendzimir galvanised

Technical data

|  |  |
| --- | --- |
| Article: | KB45H/55/110 |
| Material: | Sheet steel, Sendzimir galvanised |
| Channel dimension: | 110 mm x Array x 55 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799555827 |
| Article number: | 0055.0582 |

Manufacturer: MAICO

KB45H/55/110 45° channel elbows, horizontal