**Exhaust air silencer SDA 50**

Sound absorber for pressure side sound insulation of ERD and DRD roof fans.

With silencing elements made of water repellent and non-flammable material.

Easy installation - retrofit installation is also possible.

Technical data

|  |  |
| --- | --- |
| Article: | SDA 50 |
| Installation site: | Roof |
| Housing material: | Sheet steel, galvanised |
| Suitable for nominal size: | 500 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Article number: | 0092.0392ALT |

Manufacturer: MAICO

SDA 50 Exhaust air silencer