**Air filter, replacement ECR 12-20 G4**

Replacement air filter for ECR compact box.

Filter change is possible without tools.

Technical data

|  |  |
| --- | --- |
| Article: | ECR 12-20 G4 |
| Installation position: | vertical / horizontal |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,24 kg |
| Filter class: | ISO Coarse 80 % (G4) |
| Width: | 330 mm |
| Height: | 275 mm |
| Depth: | 45 mm |
| Width with packaging: | 331 mm |
| Height with packaging: | 276 mm |
| Depth with packaging: | 46 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799938934 |
| Article number: | 0093.0893 |

Manufacturer: MAICO

ECR 12-20 G4 Air filter, replacement