**Air filter, replacement WSF-AKF 320/470**

Active carbon filter for the WR 310/WR 410, WS 320 and WS 470 centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WSF-AKF 320/470 |
| Installation position: | vertical / horizontal |
| Weight: | 0,49 kg |
| Weight including packaging: | 0,5 kg |
| Type of filter: | Active charcoal filter |
| Filter class: | ISO ePM10 80 % (M5) |
| Width: | 507 mm |
| Height: | 166 mm |
| Depth: | 58 mm |
| Width with packaging: | 580 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 320..., WS 470..., WR 310, WR 410 |
| Range: | K |
| GTIN (EAN): | 4012799925637 |
| Article number: | 0092.0563 |

Manufacturer: MAICO

WSF-AKF 320/470 Air filter, replacement