**Push-in frame for air filter WSG-ES 320/470**

Push-in frame to position the WSG-EG 320/470 replacement air filter mats.

Technical data

|  |  |
| --- | --- |
| Article: | WSG-ES 320/470 |
| Installation position: | vertical / horizontal |
| Material: | Steel, galvanised |
| Weight: | 0,57 kg |
| Weight including packaging: | 0,58 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Width: | 505 mm |
| Height: | 170 mm |
| Depth: | 20 mm |
| Width with packaging: | 520 mm |
| Height with packaging: | 173 mm |
| Depth with packaging: | 22 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 320..., WS 470..., WR 310, WR 410 |
| Range: | K |
| GTIN (EAN): | 4012799925613 |
| Article number: | 0092.0561 |

Manufacturer: MAICO

WSG-ES 320/470 Push-in frame for air filter