**Filter locking covers WS-FVA 160**

Filter locking cover made from powder-coated sheet for WS 160 Flat centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WS-FVA 160 |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, powder coated |
| Weight: | 1,8 kg |
| Weight including packaging: | 2,07 kg |
| Width: | 375 mm |
| Height: | 190 mm |
| Depth: | 6 mm |
| Width with packaging: | 430 mm |
| Height with packaging: | 380 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 2 pieces |
| Suitable for products: | WS 160 Flat... |
| Range: | K |
| GTIN (EAN): | 4012799925651 |
| Article number: | 0092.0565 |

Manufacturer: MAICO

WS-FVA 160 Filter locking covers