**Ceiling fixing bracket WS-BWD 160**

Fixing bracket for the assembly of WS 160 Flat and WS 300 Flat centralised ventilation units on the ceiling.

The unit is acoustically isolated from the ceiling by the integrated damping element.

Technical data

|  |  |
| --- | --- |
| Article: | WS-BWD 160 |
| Installation site: | Ceiling |
| Material: | Sheet steel, galvanised |
| Weight: | 0,84 kg |
| Weight including packaging: | 0,9 kg |
| Width: | 40 mm |
| Height: | 132 mm |
| Depth: | 53 mm |
| Width with packaging: | 170 mm |
| Height with packaging: | 160 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 4 pieces |
| Suitable for products: | WS 160 Flat... |
| Range: | K |
| GTIN (EAN): | 4012799925668 |
| Article number: | 0092.0566 |

Manufacturer: MAICO

WS-BWD 160 Ceiling fixing bracket