**Compact air distributor made of plastic, 7-way MF-VK90-7**

Compact air distributor with 7 connections for MF-F90 flexible ducts.

Made from polypropylene with sound insulation (EPP).

Two service openings.

Service opening either at top or bottom.

With pre-drilled holes for installation with threaded rods.

Long working life and environmental stability.

Including 5 blind covers.

Technical data

|  |  |
| --- | --- |
| Article: | MF-VK90-7 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 160 m³/h recommended |
| Installation site: | Ceiling / Wall / Floor |
| Material: | Plastic EPP |
| Synthetic material definition: | PVC-free |
| Weight: | 0,79 kg |
| Weight including packaging: | 0,87 kg |
| Connection diameter: | 125 mm / 160 mm |
| Flexible steel duct connection diameter: | 90 mm |
| Number of couplings: | 7 |
| Width: | 300 mm |
| Height: | 217,5 mm |
| Depth: | 485 mm |
| Width with packaging: | 305 mm |
| Height with packaging: | 225 mm |
| Depth with packaging: | 492 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599944 |
| Article number: | 0059.0994 |

Manufacturer: MAICO

MF-VK90-7 Compact air distributor made of plastic, 7-way