**Shell sleeve PP 45 RHL**

Accessories needed for the PP 45 K, PP 45 O, PP 45 RC, PPB 30 K, PPB 30 O and PPB 30 RC final installation kits.

Available in two different lengths: PP 45 RHK, 500 mm in length, and PP 45 RHL, 800 mm in length.

Scope of delivery: 1 x shell sleeve, 1 x mounting material.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 RHL |
| Installation site: | Outside wall |
| Material: | Synthetic material |
| Colour: | grey |
| Weight: | 1,91 kg |
| Weight including packaging: | 2,05 kg |
| Nominal size: | 160 mm |
| Length: | 800 mm |
| Width: | 160 mm |
| Height: | 160 mm |
| Depth: | 800 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 815 mm |
| Needed core hole: | 162 mm |
| Recommended core drilling: | 182 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799590828 |
| Article number: | 0059.0082 |

Manufacturer: MAICO

PP 45 RHL Shell sleeve