**Air filter, replacement ECR 25-31 EC M5**

Replacement air filter for ECR EC compact box.

Filter change is possible without tools.

Technical data

|  |  |
| --- | --- |
| Article: | ECR 25-31 EC M5 |
| Installation position: | vertical / horizontal |
| Weight: | 0,31 kg |
| Weight including packaging: | 0,5 kg |
| Filter class: | ISO ePM10 60 % (M5) |
| Width: | 395 mm |
| Height: | 45 mm |
| Depth: | 335 mm |
| Width with packaging: | 396 mm |
| Height with packaging: | 46 mm |
| Depth with packaging: | 336 mm |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799991885 |
| Article number: | 0093.1524 |

Manufacturer: MAICO

ECR 25-31 EC M5 Air filter, replacement