**Replacement kit ER-RPK**

The replacement kit permits the reverse-compatible installation of the ER EC fan insert in existing ER - UP/G, ER - UPD and ER - UPB... housings

Comprising floor seal, blind plug, air outlet adapter, adapter board with screw and central screw.

Technical data

|  |  |
| --- | --- |
| Article: | ER-RPK |
| Weight: | 0,07 kg |
| Weight including packaging: | 0,27 kg |
| Width: | 210 mm |
| Height: | 80 mm |
| Depth: | 205 mm |
| Width with packaging: | 275 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 275 mm |
| Packing unit: | 1 set |
| Suitable for products: | ER EC |
| Range: | B |
| GTIN (EAN): | 4012799992332 |
| Article number: | 0093.1563 |

Manufacturer: MAICO

ER-RPK Replacement kit