**Push-in frame for air filter WSG-ES 300**

Push-in frame for WSG-EG 300 air filter.

Can consistently be re-used.

Is needed if the WS 300 Flat is to be equipped with an extra G4 filter in the outside air.

Technical data

|  |  |
| --- | --- |
| Article: | WSG-ES 300 |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 0,3 kg |
| Weight including packaging: | 0,32 kg |
| Width: | 320 mm |
| Height: | 245 mm |
| Depth: | 20 mm |
| Width with packaging: | 390 mm |
| Height with packaging: | 270 mm |
| Depth with packaging: | 25 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 300 Flat |
| Range: | K |
| GTIN (EAN): | 4012799992233 |
| Article number: | 0093.1326 |

Manufacturer: MAICO

WSG-ES 300 Push-in frame for air filter