**Air filter, replacement WSF-AKF 300**

Replacement air filter for WS 300 Flat... centralised ventilation units

Technical data

|  |  |
| --- | --- |
| Article: | WSF-AKF 300 |
| Installation position: | vertical / horizontal |
| Weight: | 0,47 kg |
| Weight including packaging: | 0,49 kg |
| Type of filter: | Active charcoal filter |
| Filter class: | ISO ePM2,5 ≥ 50 % (M6) |
| Width: | 320 mm |
| Height: | 245 mm |
| Depth: | 50 mm |
| Width with packaging: | 370 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 65 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 300 Flat |
| Range: | K |
| GTIN (EAN): | 4012799992257 |
| Article number: | 0093.1328 |

Manufacturer: MAICO

WSF-AKF 300 Air filter, replacement