**Summer cassette SK 150**

Summer cassette for the supply of fresh outside air without using the heat exchange process during summer operation for WS 150 ventilation unit.

Existing heat exchanger should be replaced with summer cassette.

Technical data

|  |  |
| --- | --- |
| Article: | SK 150 |
| Material: | Aluminium |
| Weight: | 6,9 kg |
| Weight including packaging: | 9,4 kg |
| Width: | 455 mm |
| Height: | 350 mm |
| Depth: | 230 mm |
| Width with packaging: | 480 mm |
| Height with packaging: | 480 mm |
| Depth with packaging: | 320 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 150 |
| Range: | K |
| GTIN (EAN): | 4012799951513 |
| Article number: | 0095.0151 |

Manufacturer: MAICO

SK 150 Summer cassette