**Air filter, replacement WSG 300-400**

Replacement air filter for WR 300 or WR 400 centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WSG 300-400 |
| Installation position: | vertical / horizontal |
| Weight: | 0,05 kg |
| Weight including packaging: | 0,27 kg |
| Filter class: | ISO Coarse 80 % (G4) |
| Width: | 410 mm |
| Height: | 170 mm |
| Depth: | 14 mm |
| Width with packaging: | 435 mm |
| Height with packaging: | 260 mm |
| Depth with packaging: | 85 mm |
| Packing unit: | 4 pieces |
| Suitable for products: | WR 300, WR 400 |
| Range: | K |
| GTIN (EAN): | 4012799938972 |
| Article number: | 0093.0897 |

Manufacturer: MAICO

WSG 300-400 Air filter, replacement