**Adjustable mounting bracket MF-FB75**

Installation aid for routing the MF-FB flexible duct with as small a bend radius as possible without damaging it.

Also serves as a mounting aid for fixing the duct's position on the wall or ceiling.

Ensures a secure hold for the flexible duct - additional means of fixing with a cable tie.

Technical data

|  |  |
| --- | --- |
| Article: | MF-FB75 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,592 kg |
| Weight including packaging: | 0,6 kg |
| Nominal size: | 75 mm |
| Angle size: | 0° - 90° |
| Step width: | 15 ° |
| Width: | 199 mm |
| Height: | 199 mm |
| Depth: | 67 mm |
| Width with packaging: | 199 mm |
| Height with packaging: | 199 mm |
| Depth with packaging: | 67 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799185635 |
| Article number: | 0018.0563 |

Manufacturer: MAICO

MF-FB75 Adjustable mounting bracket