**External grille MGR 160 alu**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

For covering round ventilation openings.

With angled lamella and bird protection grille.

With DN 160 socket for direct connection to ventilation ducts.

Technical data

|  |  |
| --- | --- |
| Article: | MGR 160 alu |
| Model: | round |
| Air direction: | Ventilation and air extraction |
| Material: | Cast aluminium |
| Weight: | 0,39 kg |
| Weight including packaging: | 0,39 kg |
| Suitable for nominal size: | 160 mm |
| Open cross section: | 120 cm² |
| Width: | 260 mm |
| Height: | 240 mm |
| Depth: | 81 mm |
| Width with packaging: | 263 mm |
| Height with packaging: | 243 mm |
| Depth with packaging: | 84 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799780366 |
| Article number: | 0078.0036 |

Manufacturer: MAICO

MGR 160 alu External grille