**External grille MGE 160 alu**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

For covering square ventilation openings.

With angled lamella and bird protection grille.

With DN 160 socket for direct connection to ventilation ducts.

Has a round connection socket with rubber sealing ring.

Technical data

|  |  |
| --- | --- |
| Article: | MGE 160 alu |
| Model: | square |
| Air direction: | Ventilation and air extraction |
| Material: | Aluminium |
| Weight: | 0,955 kg |
| Weight including packaging: | 1 kg |
| Suitable for nominal size: | 160 mm |
| Open cross section: | 180 cm² |
| Width: | 260 mm |
| Height: | 240 mm |
| Depth: | 35 mm |
| Width with packaging: | 261 mm |
| Height with packaging: | 260 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799780373 |
| Article number: | 0078.0037 |

Manufacturer: MAICO

MGE 160 alu External grille