**Mounting frame for TFA/TFZ EBR-D 10**

Mounting frame for disk valves with bayonet closure.

With thread and recessed safe sealing, exception: EBR 15.

For connecting to the duct.

Accessories needed for TFA or TFZ metal disk valves.

Technical data

|  |  |
| --- | --- |
| Article: | EBR-D 10 |
| Air direction: | Ventilation and air extraction |
| Material: | Sheet steel, galvanised |
| Colour: | galvanised |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,1 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 125 mm |
| Height: | 125 mm |
| Depth: | 50 mm |
| Width with packaging: | 125 mm |
| Height with packaging: | 125 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799924937 |
| Article number: | 0092.0493 |

Manufacturer: MAICO

EBR-D 10 Mounting frame for TFA/TFZ