**Dark room attachment ZDK 25**

Dark room attachment to screen the light at the ventilation opening.

Must be fitted inside the room.

Technical data

|  |  |
| --- | --- |
| Article: | ZDK 25 |
| Air direction: | Air extraction |
| Installation: | Inside |
| Installation site: | Wall / Ceiling |
| Type of installation: | Surface-mounted |
| Material: | Sheet steel, powder coated |
| Colour: | Black |
| Weight: | 8,56 kg |
| Weight including packaging: | 10,2 kg |
| Width: | 483 mm |
| Height: | 483 mm |
| Depth: | 254 mm |
| Width with packaging: | 585 mm |
| Height with packaging: | 505 mm |
| Depth with packaging: | 280 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799933502 |
| Article number: | 0093.0350 |

Manufacturer: MAICO

ZDK 25 Dark room attachment