**Flexible coupling ELA 31 Ex**

Flexible couplings for the sound and vibration damped connection of ventilation ducts.

With flanges fitted on the fan side.

With push-in couplings on the duct side.

ELA ..: Made of plastic.

ELA .. Ex: Made of antistatic material, for use in areas subject to explosion hazards.

Technical data

|  |  |
| --- | --- |
| Article: | ELA 31 Ex |
| Flange material: | Steel, galvanised |
| Cuff material: | Synthetic material, antistatic |
| Weight: | 2,15 kg |
| Weight including packaging: | 2,2 kg |
| Suitable for nominal size: | 315 mm |
| Width: | 380 mm |
| Height: | 380 mm |
| Depth: | 220 mm |
| Width with packaging: | 381 mm |
| Height with packaging: | 381 mm |
| Depth with packaging: | 221 mm |
| Ex version: | antistatic |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799922858 |
| Article number: | 0092.0285 |

Manufacturer: MAICO

ELA 31 Ex Flexible coupling