**Flexible coupling ELP 50**

Flexible couplings for mounting channel fans that are free from structure-borne noise.

With square flange connection frames made of galvanised steel.

Installation on the inlet and outlet sides.

Technical data

|  |  |
| --- | --- |
| Article: | ELP 50 |
| Installation site: | Channel |
| Material: | Synthetic material |
| Weight: | 3,54 kg |
| Weight including packaging: | 4,04 kg |
| Channel dimension: | 800 mm x 500 mm |
| Width: | 840 mm |
| Height: | 540 mm |
| Depth: | 150 mm |
| Width with packaging: | 865 mm |
| Height with packaging: | 580 mm |
| Depth with packaging: | 75 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799921233 |
| Article number: | 0092.0123 |

Manufacturer: MAICO

ELP 50 Flexible coupling