**Connection frame ZVR 50**

Connection frames for mounting the AS and RS shutters to the fan models of EZQ, EZS, DZQ and DZS series.

For fitting in thin walls.

Technical data

|  |  |
| --- | --- |
| Article: | ZVR 50 |
| Installation: | outside |
| Installation site: | Thin wall |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 2,17 kg |
| Weight including packaging: | 2,2 kg |
| Suitable for nominal size: | 500 mm |
| Width: | 578 mm |
| Height: | 578 mm |
| Depth: | 2 mm |
| Width with packaging: | 578 mm |
| Height with packaging: | 578 mm |
| Depth with packaging: | 2 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799931973 |
| Article number: | 0093.0197 |

Manufacturer: MAICO

ZVR 50 Connection frame