**Pressure tubing Centro-PP**

Can be used with MAICO Centro centralised ventilation system.

Negative pressure hose for connecting the measuring lance to the pressure cell.

Easy plug-in connection without clips.

Technical data

|  |  |
| --- | --- |
| Article: | Centro-PP |
| Material: | Synthetic material |
| Colour: | Blue |
| Weight: | 0,17 kg |
| Weight including packaging: | 0,2 kg |
| Internal diameter: | 6 mm |
| External diameter: | 8 mm |
| Length: | 5 m |
| Width: | 5.000 mm |
| Height: | 8 mm |
| Depth: | 8 mm |
| Width with packaging: | 300 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 15 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799924876 |
| Article number: | 0092.0487 |

Manufacturer: MAICO

Centro-PP Pressure tubing