**Accessories for glass brick walls ZG 31**

Mounting frame for assembly of window fans in glass brick walls.

Consisting of window putty, screws and cover plate.

Pane thickness up to 100 mm.

Technical data

|  |  |
| --- | --- |
| Article: | ZG 31 |
| Installation site: | Glass brick |
| Weight: | 1,7 kg |
| Weight including packaging: | 2,14 kg |
| Width: | 440 mm |
| Height: | 440 mm |
| Depth: | 1 mm |
| Width with packaging: | 470 mm |
| Height with packaging: | 450 mm |
| Depth with packaging: | 35 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799931584 |
| Article number: | 0093.0158 |

Manufacturer: MAICO

ZG 31 Accessories for glass brick walls