**Room sensor FR 30 P**

Temperature sensor for measuring the air temperature in enclosed areas.

Can be combined with ETL 16 P, DTL 16 P, DTL 24 P.

Technical data

|  |  |
| --- | --- |
| Article: | FR 30 P |
| Degree of protection: | IP 20 |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,08 kg |
| Weight including packaging: | 0,09 kg |
| Width: | 86 mm |
| Height: | 86 mm |
| Depth: | 30 mm |
| Width with packaging: | 98 mm |
| Height with packaging: | 98 mm |
| Depth with packaging: | 37 mm |
| Temperature setting range: | 0 °C up to 30 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799577812 |
| Article number: | 0157.0781 |

Manufacturer: MAICO

FR 30 P Room sensor