**Axial duct fan DZR 35/4 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZR 35/4 A-Ex |
| Air flow volume: | 2.800 m³/h |
| Rotating speed: | 1.390 1/min |
| Nominal output: | 165 W |
| Inom: | 0,47 A |
| Imax: | 0,54 A |
| Weight: | 12,2 |
| IA/IN: | 3,4 |
| Certified as explosion proof: | 84/3892 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799867715 |
| Article number: | 0086.0771 |

Manufacturer: MAICO

DZR 35/4 A-Ex Axial duct fan