**Axial duct fan DZR 45/6 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZR 45/6 A-Ex |
| Air flow volume: | 4.500 m³/h |
| Rotating speed: | 960 1/min |
| Nominal output: | 200 W |
| Inom: | 0,64 A |
| Imax: | 0,61 A |
| Weight: | 16,4 |
| IA/IN: | 2,6 |
| Certified as explosion proof: | 84/3896 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799867807 |
| Article number: | 0086.0780 |

Manufacturer: MAICO

DZR 45/6 A-Ex Axial duct fan