**Axial roof fan DZD 25/2 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 25/2 A-Ex |
| Air flow volume: | 1.700 m³/h |
| Rotating speed: | 2.835 1/min |
| Nominal output: | 200 W |
| Inom: | 0,36 A |
| Imax: | 0,36 A |
| Weight: | 17,6 |
| IA/IN: | 4,9 |
| Certified as explosion proof: | 84/3885 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799877615 |
| Article number: | 0087.0761 |

Manufacturer: MAICO

DZD 25/2 A-Ex Axial roof fan