**Axial roof fan DZD 35/6 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 35/6 A-Ex |
| Air flow volume: | 1.370 m³/h |
| Rotating speed: | 985 1/min |
| Nominal output: | 115 W |
| Inom: | 0,62 A |
| Imax: | 0,67 A |
| Weight: | 28,6 |
| IA/IN: | 2,6 |
| Certified as explosion proof: | 84/3890 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799877707 |
| Article number: | 0087.0770 |

Manufacturer: MAICO

DZD 35/6 A-Ex Axial roof fan