**Airstream limiter VSB 125**

Volumetric flow limiter for ventilation units and exhaust air systems.

Simple feeder in DN 100 and/or DN 125 ducts.

High level of control accuracy.

Maintenance-free.

Can be operated in any position.

Quick and easy to set.

Technical data

|  |  |
| --- | --- |
| Article: | VSB 125 |
| Pressure range: | 30 Pa - 300 Pa |
| Volumetric flow: | 40 m³/h - 205 m³/h |
| Installation position: | any |
| Housing material: | Synthetic material |
| Weight: | 0,14 kg |
| Weight including packaging: | 0,15 kg |
| Nominal size: | 125 mm |
| Width: | 120 mm |
| Height: | 120 mm |
| Depth: | 115 mm |
| Width with packaging: | 121 mm |
| Height with packaging: | 121 mm |
| Depth with packaging: | 116 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799931102 |
| Article number: | 0093.0110 |

Manufacturer: MAICO

VSB 125 Airstream limiter