**Slide-in adaptor MF-WE75**

The slide-in adaptor is needed to establish a perfect coupling between the MF-F flexible steel duct and MF-W or MF-WL bracket.

The MF-F flexible steel duct is quickly and securely linked to the slide-in adaptor using the "click principle".

Scope of delivery: Slide-in adaptor including a plug.

Accessories needed: Two MF-FDR gaskets.

Technical data

|  |  |
| --- | --- |
| Article: | MF-WE75 |
| Air direction: | Ventilation and air extraction |
| Material: | Polypropylene (PP) |
| Synthetic material definition: | PVC-free |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,13 kg |
| Nominal size: | 75 mm |
| Width: | 199,5 mm |
| Height: | 79,5 mm |
| Depth: | 67,5 mm |
| Width with packaging: | 199,5 mm |
| Height with packaging: | 79,5 mm |
| Depth with packaging: | 67,5 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599722 |
| Article number: | 0059.0972 |

Manufacturer: MAICO

MF-WE75 Slide-in adaptor