**Bypass for heat exchanger WS-BP 160**

Automatic 100 % bypass with position feedback for the WS 160 Flat centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WS-BP 160 |
| Weight: | 0,6 kg |
| Weight including packaging: | 0,9 kg |
| Width: | 170 mm |
| Height: | 160 mm |
| Depth: | 80 mm |
| Width with packaging: | 171 mm |
| Height with packaging: | 161 mm |
| Depth with packaging: | 81 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 160 Flat... |
| Range: | K |
| GTIN (EAN): | 4012799925699 |
| Article number: | 0092.0569 |

Manufacturer: MAICO

WS-BP 160 Bypass for heat exchanger